**Standard press seal**

with continuously variable super segment ring technology

Article Code: HSD SSG

GTIN: -

Brand: Hauff-Technik

Split annular space seal for the continuous sealing of newly installed or already installed pipes in core drill holes or casing pipes. Tested according to FHRK test basis with FHRK quality seal.

Dimensions: Sealing width up to Ø 250 mm: 40 mm; Sealing width for Ø 300 mm: 50 mm

Material: Press plates, screws and nuts: rust-free stainless steel V2A (AISI 304L) or V4A (AISI 316L); Rubber: EDPM or NBR

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight; radon-proof

Features: Visual and physical installation control thanks to integrated inspection opening; integrated super segmented ring technology for individual adjustment to cable/pipe diameter on site; Segments with diameter marking

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de