**Outer sealing element module 6**

for district heating basic variant 1 and 2

Article Code: MSH FW Basic M6

GTIN: -

Brand: Hauff-Technik

For sealing in core drills for double walls/element walls. The sealing width of 90 mm provides a seal against both the concrete shells of the double/element wall and the pre-mixed concrete filling.

Dimensions: Compatible with core drill/wall sleeve ID: 299 - 302 mm; Sealing width: 90 mm; Insertion depth: 115 mm

Material: Die-cast aluminium with cathodic coating/EPDM

Application range: Waterproof concrete stress class 1 and 2

Features: visual installation reliability due to built-in inspection opening

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de