**Standard press seal**

Article Code: HSD100 RW 1x25/32/40+3x6-18 b40 A2/EPDM

GTIN: -

Brand: Hauff-Technik

Split press seal for sealing new media pipes/cables to be installed or media pipes/cables that have already been laid in core drills or wall sleeves. Tested according to FHRK test basis with FHRK quality seal.

Dimensions: Sealing width: 40 mm; For core drills/wall sleeves Ø: 100 mm; For 4 cables/pipes of which 3 x Ø 6-18 mm and 1 x Ø 25, 32 or 40 mm

Material: Press plates, screws and nuts: rust-free stainless steel V2A (AISI 304L); Rubber: EPDM

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight; radon-proof

Features: Visual and physical installation control thanks to integrated inspection opening; integrated segmented ring technology for individual adjustment to cable diameters on site

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de