**Single wall insert with plug-in socket**

adjustable length, for setting in concrete and connecting smooth cable ducts

Article Code: HSI150 GSM Varia

GTIN: -

Brand: Hauff-Technik

Single wall insert with plug-in socket. The square connection frame for system seals can be used to create packages for installation flush with formwork on site (spacers must be used for cable ducts ∅ 160 mm), additional pipe connectors are not necessary.

Dimensions: Minimum wall thickness OD 110, 125mm: 200 mm; Minimum wall thickness OD 160mm: 260 mm; Centre distance: 210 mm, spacer increases centre distance to 250 mm; Frame dimensions: 220x 220 mm

Material: Wall insert: ABS with TPE 3-ribbed seal; Adapter pipe: PVC; Clamping strap: Steel St sn (W1); Closing cover: ABS with TPE seal; Plug-in socket: EPDM; Clamping strap for HSI150 GSM160/X: W4; Pipe cover: PE or end plug: PVC

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 0.5 bar; radon-proof

Features: stepless adjustment to the required wall thickness on site; injection molded 3-ribbed seal for pressure-tightness seal with concrete; Quality seal: tightness from the factory. Option to check for accidental or unauthorized opening of the closing cover

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de