**Universal wall entry**

without edges

Article Code: UDM

GTIN: -

Brand: Hauff-Technik

Wastewater wall entry for setting in concrete in the wall. With plug-in socket moulded on one side and 3-ribbed seal as a water barrier.

Dimensions: DN 110: minimum wall thickness 200 mm; DN 150: minimum wall thickness 240 mm

Material: Rubber sleeve: EPDM; Sleeve cover: ABS; Clamping strap: Steel St sn (W1); Lamella plugs: PE; KG pipe: PVC-U/KG2000 pipe: PP

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight; radon-proof

Tests/Standards: KG2000 pipes to DIN EN 14758; KG pipes to DIN EN 13476-2

Features: with integrated flange to connect foils; no change in flow direction; pressure-sealed after concreting

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de