**Cement-coated wall sleeve with sleeve**

floor entry for Hateflex spiral hose

Article Code: KES MA90 ZVR100/500

GTIN: -

Brand: Hauff-Technik

Cement-coated wall sleeve with sleeve Cable duct system in the form of a floor slab entry system with break-resistant, inherently stable cement-coated wall sleeve for the connection of the Hateflex 14090 spiral hose with the sleeve method.

Dimensions: Wall sleeve ID: 100 mm; Length (excluding sleeve): 500 mm

Material: Pipe: PVC-U; Closing cover: PE; Sleeve: EPDM; Clamping straps: W4

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight

Features: special coating creates a homogeneous bond with the concrete; The cement-coated pipe can be cut to size straight or at an angle once the floor has been finished

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de