**Compensating pipe seal**

with segmented rings

Article Code: ADM

GTIN: -

Brand: Hauff-Technik

Closed sealing sleeve for dowel-fitting/screwing down to outside of building/housings with existing wall sleeves, break-throughs or concrete core drills for sealing new media pipes/ducts to be installed.

Dimensions: Flang all around: 30mm; Outer diameter ADM150: 290 mm; Outer diameter ADM200: 340 mm

Material: Sealing sleeve: EPDM; Fixing ring: stainless steel V2A (AISI 304L); Clamping straps: stainless steel V2A (AISI 304L); Fastenings: stainless steel V4A (AISI 316L)

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight

Features: absorption of radial and axial movements; Segmented ring technology for adjustment on-site to pipe diameters

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de