**Tundish**

Article Code: AT110

GTIN: -

Brand: Hauff-Technik

Tundish with integrated step protection for setting in floor slab concrete for perfect sealing to the underground sewer pipe. Gastight and watertight connection to the floor slab using integrated 3-ribbed seal. Gastight and watertight connection to the KG pipe using TPE-seal. To compensate an offset (after concreting) between downpipe and floor drain in any direction.

Dimensions: Offset diameter: 250 mm; Flange all around: 50mm; for underground sewage pipe Ø 110 mm

Material: Step protection: PP; Tundish: ABS/TPE; Profile sealing: TPE; Clamping strap: Steel St sn (W4)

Application range: Water exposure class DIN 18533: W1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight; radon-proof

Tests/Standards: KG pipes to DIN EN 13476-2; KG2000 pipes to DIN EN 14758

Features: with axial tolerance compensation; easy integration of the vapour barrier using the adhesive flange; non-trip installation according to DGUV 38 §12a thanks to step protection; With integrated level for positioning the tundish

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de