**Membrane injection system**

for buildings with a basement

Article Code: MIS90D

GTIN: -

Brand: Hauff-Technik

For installation in all standard wall types to DIN 18533 and waterproof concrete to DIN 1045. Including wall end rosettes and sleeve plugs.

Dimensions: For core drills ID: 92 - 102 mm

Material: Flange, counter-bearing, sleeve cap, wall rosette, membrane hose: EPDM; Resin injection hose: PE; Pipe: PVC-U; Sealing tape: butyl; Stainless steel clamping straps: V2A (AISI 304L)

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 1.0 bar

Features: universal building entry with membrane injection system for core holes in the most common types of wall; Controlled resin discharge through slotted membrane hose; simultaneous sealing of power, water and communication services

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de