**Double wall insert with flange connection**

for setting in concrete

Article Code: HSI150 1xZ K2 AF/X

GTIN: -

Brand: Hauff-Technik

Double wall insert with flange connection for installation flush with formwork, used for the gastight and watertight connection on both sides of system seals for cables and cable ducts, packages can be created with frame system, delivery ex works. Tested according to FHRK test basis with FHRK quality seal.

Dimensions: Frame dimensions 1x1 package configuration: 340 x 340 mm; Frame dimensions 1x4 package configuration: 970 x 340 mm; Minimum wall thickness 140 mm

Material: Wall insert: ABS with TPE 3-ribbed seal; Adapter pipe: PVC; Closing cover: ABS with TPE seal; Flange: ABS

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 2.5 bar; radon-proof

Features: Flange for plastic-modified bitumen thick coatings; Tested solution for use in pre-applied membrane sheet systems; 1x1 or 1x4 package arrangement; Quality mark on both sides: factory-sealed. Option to check for accidental or unauthorized opening of the closing cover

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de