**basic component**

Fibre optic handover system

Article Code: 2LINE G-BOX GBT

GTIN: -

Brand: Hauff-Technik

Prepared with fitted plastic cover, 2 triangular safety screws, cover seal and height-adjustable top section to adapt to the ground level. Make: Hauff-Technik

Dimensions: Overall height: 480 - 580 mm; Lid dimensions: 157 x 157 mm; Height adjustment: 100 mm

Material: Cast lid: EN-GJL-250 (GG25); Plastic lid: glass fibre reinforced polyamide (PA-GF); Top section: glass fibre reinforced polyamide (PA-GF); Bottom section: ABS; Screws: stainless steel V2A (AISI 304L)

Tests/Standards: Manufactured in accordance with DIN 3580; In accordance with DVGW VP310-2; Verified lid load: 20 metric tons (cast); Verified lid load: 12.5 metric tons (plastic)

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de