**DiSan**

granulated, mineral sand sealant

Article Code: DiSan

GTIN: -

Brand: Hauff-Technik

Granulated, mineral sand sealant as a renovation solution for subsequent waterproofing of substations.

Material: mineral compound made from various sands and bentonite with optimal grain size 0/2 mm

Features: after contact with water it forms a highly plastic mixture, which provides a durable sealant for exterior areas.

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de