**Membrane injection system**

for buildings with a basement

Article Code: MIS40D

GTIN: -

Brand: Hauff-Technik

For installation in all standard wall types to DIN 18533 and waterproof concrete to DIN 1045. Incl. wall rosettes, tubular guide elbows, 2-component resin iM3000. 1 piece mounting tool per packing unit.

Dimensions: For core drills ID: 40 - 50 mm

Material: Flange and counter-bearing EPDM; Resin injection hose: PE; Sealing tape: butyl; Pipe: PVC-U; Wall terminator element: Flame-retardant polycarbonate; Quick tensioning device: glass fibre reinforced polyamide/ABS

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 1.0 bar

Features: universal building entry with membrane injection system for core holes in the most common types of wall; Controlled resin discharge through slotted membrane hose; sealing lips ensure gentle seal for cables/pipes

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de