**Membrane injection system**

for buildings without a basement

Article Code: MIS40S

GTIN: -

Brand: Hauff-Technik

For sloping entry through the wall or floor slab in all common types of wall in load case DIN 18533 and waterproof concrete to DIN 1045. Incl. wall rosettes, tubular guide elbows, 2-component resin iM3000. 1 piece mounting tool per packing unit.

Dimensions: For core drills ID: 40 - 50 mm; Overall length: 1300 mm

Material: Flange and counter-bearing EPDM; Resin injection hose: PE; Pipe: PVC-U; Wall terminator element: Flame-retardant polycarbonate; Quick tensioning device: glass fibre reinforced polyamide/ABS

Application range: Water exposure class DIN 18533: W1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 1.0 bar

Features: universal building entry with membrane injection system for core holes in the most common types of wall; Controlled resin discharge through slotted membrane hose; sealing lips ensure gentle seal for cables/pipes

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de