**Fixed/loose flange wall sleeve galvanised**

For setting in concrete and connecting bituminous coating

Article Code: FLFE DIN18533 St-A3C

GTIN: -

Brand: Hauff-Technik

For setting in concrete or mortaring into walls, ceilings or floors.

Dimensions: for wall thicknesses of up to 500 mm; Design in accordance with DIN 18533 includes: components in contact with the soil; Standard fixed flange Øa equal to the relevant wall sleeve Øi + approx. 330 mm (for one passage)

Material: Fixed/loose flange wall sleeve steel galvanised (gv); Wall sleeve: plastic PVC-U; Closing cover: PE; Bolts and nuts: steel galvanised (gv)

Application range: Water exposure class DIN 18533: W1-E, W2.1-E and W2.2-E

Tightness: gastight and watertight

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de