**Fixed/loose flange wall sleeve galvanised**

for retrofit dowelling for black tank

Article Code: FLFA DIN18533 A3C

GTIN: -

Brand: Hauff-Technik

For fixing in front of wall sleeves, core drills or breakthroughs.

Dimensions: Standard upper length: 80 mm; Design in accordance with DIN 18533 includes: components in contact with the soil; Standard fixed flange Øa equal to the relevant wall sleeve Øi + approx. 330 mm (for one passage)

Material: Fixed/loose flange wall sleeve steel galvanised (gv); Fastenings: stainless steel V4A (AISI 316L); Nuts: Steel galvanised (gv)

Application range: Water exposure class DIN 18533: W1-E, W2.1-E and W2.2-E

Tightness: gastight and watertight

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de