**Seal insert for basic insert**

arranged side by side

Article Code: MSH Basic MBK R4

GTIN: -

Brand: Hauff-Technik

For the collective feeding in and sealing of all supply lines (power, water, telecommunications, gas) for buildings without a basement, for installation in MSH Basic - FUBO - E - SR 4 wall sleeve. The MSH Basic - MBK - R4 is supplemented with an MSH sealing elements set which is available to purchase separately.

Dimensions: Width: 500 mm; Length: 135 mm; Height: 283 mm

Material: Anchor plate: glass fibre reinforced polyamide; Pipes: ABS with TPE; Screws: stainless steel V2A (AISI 304L)

Tightness: gastight and watertight to 1.0 bar

Tests/Standards: DVGW VP 601

Features: all-around smooth surface for optimum connection of the finished flooring

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de