**ETGAR building package for multi-line building service outlets**

for buildings with a basement

Article Code: HAW-M ETGAR BHP

GTIN: -

Brand: Hauff-Technik

For routing and distributing electric power and communication lines from the building to the property's surrounding grounds.

Dimensions: Compatible with ETGAR wall sleeve, ID: 200 mm; maximum wall thickness: 500 mm

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 1.0 bar

Features: complete system for distributing the power supply to the entire property from the building connection room; integrated leak test equipment

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de