**ETGAR wall sleeve for building services outlet**

for ETGAR BHP

Article Code: HAW-M ETGAR FR

GTIN: -

Brand: Hauff-Technik

For installation flush to the formwork into all common wall types. With spigot flange and three 3-web gaskets (e.g. as water barrier in double/element walls).

Dimensions: minimum wall thickness: 200 mm; Maximum wall thickness: 400 mm

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de