**Connection wall sleeve**

Article Code: AFR 100

GTIN: -

Brand: Hauff-Technik

Wall sleeve for easy installation in formwork, sealed on both sides ready for installation for flush setting in concrete. For the direct connection of a smooth duct DN 110 with plug-in/glue-in socket.

Material: Rubber sleeve: EPDM; Sleeve cover: ABS; Clamping strap: Steel St sn (W1); Closing cover: PE; Pipe: PVC-U

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight; radon-proof

Features: integrated flange connection; pressure-sealed after concreting

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de