**Polymer flange**

Material: Flange: glass fibre reinforced polyamide; Surface seal: EPDM; Fastenings: stainless steel V4A (AISI 316L)

: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1, waterproof concrete stress class 2

Tightness: gastight and watertight to 2.5 bar

Features: with integrated spirit level; tried and tested solution for use in fresh concrete composite systems

Article Code: HSI150 DFK

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de