**Single-line building entry ZAPPO**

Material: Front panel and twist protection flaps: Fibre glass reinforced polyamide; Rubber: EPDM; Rear press ring and outer sealing element: stainless steel V2A (AISI 304L); Centring ring: stainless steel V2A (AISI 304L); Screws: stainless steel V2A (AISI 304L); Screws: stainless steel V2A (AISI 304L)

: Water exposure class DIN 18533: W1-E; Waterproof concrete stress class 1, waterproof concrete stress class 2

Tightness: gastight and watertight to 1.0 bar

Tests/Standards: DVGW VP 601

Features: no groundwork at the property; continuous gastight empty conduit system

Article Code: ESH PolySafe VT75

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de