**Individual press seal**

with segmented ring technology

For use in wall insert and plastic flange HSI150. Split design for sealing new cables to be installed or cables that have already been laid and various frequently recurring cable configurations. The individual seal with segmented rings enables the cable diameter to be adjusted on site. A number of individual seals can be replaced by a single universal seal.

Dimensions: Sealing width: 60 mm; Press plates: 5 mm; OD: 150 /160 mm

Material: Press plates, screws, nuts and washers: rust-free stainless steel V2A (AISI 304L) or V4A (AISI 316L); Rubber: EPDM

Tightness: gastight and watertight; radon tight

: Tailor-made to meet requirements; Segmented ring technology for adjustment to three or five different pipe diameters on site; Form-locked connection to bayonet, therefore integrated tear-out protection; Also suitable for sealing TRI-Delta cables

: HRD150/160 SGi b60

GTIN: -

**Hauff-Technik GmbH & Co. KG**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de