**Two-level fixed/loose flange**

for setting in concrete

Wall sleeve with 2 fixed/loose flanges for setting in concrete on insulated flat roofs with two waterproof membranes to DIN 18531.

Dimensions: Design according to DIN 18531 includes: DIN 18531 (roofs), DIN 18532 (areas for vehicles), DIN 18534 (interiors), DIN 18535 (containers).; Standard fixed flange Øa equal to the relevant wall sleeve Øi + approx. 150 mm (for one passage, see brochure for details)

Material: Stainless steel V2A (AISI 304L) or V4A (AlSI 316L)

Tightness: gastight and watertight

Article Code: 2FLFE DIN18531

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de