**Outer sealing element module 1.2**

Material: Fibre glass reinforced polyamide / EPDM

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Features: tested according to DIN 18533; visual installation reliability due to built-in inspection opening

Article Code: MSH PolySafe M1.2

Article number: 1560000104

GTIN: 4052487162784

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de