**Wall entry pipe bend 160**

for district heating lines

Article Code: MSH Basic FUBO-FIX RB160 r1000

Article number: 1900500160

GTIN: 4052487157438

Brand: Hauff-Technik

For the feeding in and sealing of district heating supply lines through the floor slab. Positioning with separately available clip system on the district heating installation fixture and combination with spiral hose system and sealing elements.

Dimensions: Pipe bend radius: max. 1,000 mm

Material: PVC

: Water exposure class DIN 18533: W1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de