**Sleeve cap and pipe connection set**

for multi-line building entry systems (wall entries)

For connecting an empty conduit route DN 75 (corrugated) to the multi-line building entry system as well as for sealing media lines on the earth side.

Dimensions: Area of application MS 78 - U: 1 cable/pipe OD 24 - 52 mm; Area of application MS 78 - KD: 1 cable OD 13 - 21 mm, 3 cables OD 7 - 13 mm, 1 cable OD 5 - 13 mm

Material: Sleeves: EPDM; Clamping straps: stainless steel V2A (AISI 304L); Double sleeves: PE-HD; Profile seal: EPDM

Features: With segmented ring technology for maximum area of application

Article Code: MSH ZBS4

Article number: 1552002130

GTIN: 4052487165877

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de