**Universal sealing element communication**

for single-line and multi-line building entry systems

Dimensions: Area of application: 1 cable OD 13 - 21 mm, 3 cables OD 7 - 13 mm, 1 cable OD 5 - 13 mm

Material: Fibre glass reinforced polyamide / EPDM

Features: With segments for maximum area of application

Article Code: SDK 1x13-21+3x7-13+1x5-13

Article number: 1560000506

GTIN: 4052487162951

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de