**Outer flange module 2**

for district heating multi-line building entry system basic variant 1 and 2

Extension module for district heating multi-line building entry system in conjunction with the MSH-FW outer sealing element module 1 or module 6. For the integration of existing building seals.

Dimensions: OD: 380 mm

Material: Flange: stainless steel V2A (AISI 304L); Profile seal: EPDM

Load case: Waterproof concrete stress class 1

Article Code: MSH FW Basic M2

Article number: 1933005100

GTIN: 4052487126625

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de