**Universal insulating plate module 3**

for district heating multi-line building entry system basic variant 1 and 2

For insertion in existing perimeter insulation, combined with MSH-FW outer sealing element module 1, module 5 or module 6.

Dimensions: OD: 440/299 mm; Insulation thickness: 50 mm

Material: Styrodur (EPS)

Features: Predetermined breaking point ensures compatibility for use with various diameters

Article Code: MSH FW Basic M3

Article number: 1933005200

GTIN: 4052487126632

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de