**Combined building entry for water DN 150**

for buildings with a basement

Combined building entry for water manufactured by Schuck, DN 150, for use in core drills or wall sleeves ID 250 mm.

Dimensions: Core drill/wall sleeve ID: 250 mm; Wall thickness: 240 - 700 mm

Material: Seal insert: stainless steel V2A (AISI 304L); Rubber: EPDM

Load case: Waterproof concrete stress class 2; Waterproof concrete stress class 1

Tightness: gastight and watertight to 1.0 bar

Article Code: ROKA WF-TE-ARO-DN150/160-PN16 BL1120

Article number: 1990800095

GTIN: 4052487054478

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de