**Combined building entry for water**

for buildings without a basement

Combined building entry for water manufactured by Schuck, DN 80, for use in basic insert part ADS 100 - FUBO - DN 80.

Dimensions: Seal insert OD: 150 mm

Material: Seal insert: stainless steel V2A (AISI 304L); Rubber: EPDM

Load case: Waterproof concrete stress class 2; Waterproof concrete stress class 1

Tightness: gastight and watertight to 1.0 bar

Item: Gebäudeeinführung Wasser

Article Code: HSFLEX WF-PE-ARO DN80/DPE90 BL4970

Article number: 1990800110

GTIN: 4052487054508

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de