**Standard press seal**

Material: Press plates, screws and nuts: rust-free stainless steel V2A (AISI 304L); Rubber: EPDM

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight; radon tight

Features: optical and tangible installation security due to integrated control opening; integrated segmented ring technology for individual adjustment to cable diameters on site

Article Code: HSD100 EW 1x24-44+4x7-12 b40 A2/EPDM

Article number: 3030300054

GTIN: 4052487126250

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de