**Basic component**

For ETGAR BHP

For creating distribution and terminal points on the property. Accessory for the ETGAR building services outlet and for the extension set.

Dimensions: Overall height: 480 - 580 mm; Lid dimensions: 157 x 157 mm; Height adjustment: 100 mm

Material: Plastic lid: glass fibre reinforced polyamide (PA-GF); Top section: glass fibre reinforced polyamide (PA-GF); Bottom section: ABS; Screws: stainless steel V2A (AISI 304L)

Tests/Standards: Verified lid load: 12.5 metric tons (plastic)

Item: ETGAR Abschluss-Box

Article Code: ETGAR AB

Article number: 3030407683

GTIN: 4052487231954

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de