**Fire protection kit S90**

for HSI150 press seal

Fire protection kit for installation in the HSI150 system for walls. No additional wall attachments, no limits on individual cable diameters, weatherproof.

Dimensions: Wall thickness at and above: 150 mm; Barrier thickness: min. 280 mm; Maximum package size: 430 x 1270 mm (2x6)

Tests/Standards: DIBT approval Z-19.15-1906 to DIN 4102-9

Wall sleeve/core drilled hole ID (mm): 150

Features: Fire protection S90 combined with HRD 150/160 press seal; Special assembly pockets for the assembly of pads on one side

Article Code: HSS150 HSI150 HRD

Article number: 5030010031

GTIN: 4052487233583

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de