**System cover**

with sleeve method for corrugated cable ducts

System cover. Seal is both mechanically stable and elastic.

Material: System cover: polycarbonate; Clamping nut: PC/PBT blend; Sleeve: EPDM; Clamping straps: W4; Ring clips: stainless steel

Tightness: gastight and watertight to 0.5 bar

Features: Mechanical fixing (bayonet) and seal (clamping nut) act independently; Bayonet system with return lock and locking screw connection (for protection against automatic opening); Patented ring clip method

Article Code: HSI90 MA WR

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de