**System cover**

with cold shrink-fit method for corrugated cable ducts

For use in wall insert and aluminium flange HSI90. For connecting corrugated cable ducts. The cold shrink sleeves support a wide area of application. They are shrunk onto the cables by the system cover socket without tools. Particularly gentle for thin-walled or temperature-sensitive pipes.

Dimensions: For pipe diameter: OD: 75 mm

Material: System cover: polycarbonate; Clamping nut: PC/PBT blend; Shrink tubing: EPDM

Tightness: gastight and watertight to 0.5 bar

Features: Mechanical fixing (bayonet) and seal (clamping nut) act independently; Bayonet system with return lock and locking screw connection (for protection against automatic opening)

Article Code: HSI90 D1x75 KS WR

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de