**Sealing Bag**

with self inflating system

For sealing cables in core drills or wall sleeves. Suitable for sealing new cables to be installed or cables that have already been laid.

Material: Aluminium plate, polyethylene and polyester; Sealing tape: butyl

Application range: Water exposure class DIN 18533: W1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 0.5 bar

Features: Patented technology for a very fast finished installation; No tools required for installation - no compound injection unit or compressed gas capsules; Highly adaptable to different line shapes and diameters

Article Code: OKT

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de