**Spiral hose**

for building entries

The Hateflex spiral hose is a flexible and very stable cable duct with a smooth inner surface for gentle cable draw-in. A pressure-tight cable entry system can be created with the associated connection components. Spiral hose with high mechanical load capacity, abrasion resistant, weatherproof, inherently stable and non-buckling.

Dimensions: Øi: 78 mm; Øa: 87 mm

Material: Hard PVC/soft PVC

Tightness: gastight and watertight to 2.5 bar

Features: Pressure-tight flexible empty conduit system (external pressure 2.5 bar) with a smooth inner surface for gentle cable draw-in

Article Code: Hateflex14078/x

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de