**ETGAR carrier plate**

for ETGAR foundation box

For mounting on the ETGAR foundation box and for versatile, safe and reliable installation of outdoor garden lighting, multi-socket power-outlet strips, and electric power charging stations, etc.

Dimensions: Diameter: 270 mm; Height: 50 / 30 mm; Diameter of predetermined breaking point: 40 mm

Material: Carrier plate: polymer concrete; Screws: stainless steel V2A (AISI 304L)

Features: Ready-to-connect foundation system for installation of electrical terminal devices

Article Code: ETGAR FB TPL

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de