**ETGAR connection sleeve**

for ETGAR foundation box

For ETGAR building services outlets and for sealing media lines on the earth side at the end of the empty conduit route DA 75 mm.

Dimensions: Area of application: 1 cable OD 13 - 21 mm, 3 cables OD 7 - 13 mm, 1 cable OD 5 - 13 mm

Material: EPDM

Features: With segments for maximum area of application

Article Code: ETGAR ANS 4x5-25

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de