**System cover**

cable seal with hot shrink-fit method

System cover. The thermal sleeves support a wide area of application, they are shrunk onto the cables by means of the application of heat from the system cover socket. Tested according to FHRK test basis with FHRK quality seal.

Material: System cover with socket: polycarbonate; Clamping nut: PC/PBT blend; Thermal sleeve with hot-melt adhesive: polyolefin; Centring strap: EPDM

Tightness: gastight and watertight to 2.5 bar

Features: Mechanical fixing (bayonet) and seal (clamping nut) act independently; Bayonet system with return lock and locking screw connection (for protection against automatic opening)

Article Code: HSI150 D WS

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de