**Universal charging station foundation**

for the installation of charging stations and charging pedestals

Article Code: ULF

GTIN: -

Brand: Hauff-Technik

Universal foundation solution for installing charging stations and charging pedestals. Option for mounting on polymer concrete slab. Connection of power and data cables via an empty pipe connection.

Dimensions: Total length: 750mm; Foundation slab: ULF300: 300 x 300 mm, ULF380: 380 x 380 mm, ULF470: 470 x 470 mm; High foundation slab: 80 mm; Foundation slab opening: ULF300/380: 110 mm, ULF470: 110/150 mm; Foundation pipe (Øi): ULF300: DN 200, ULF380: DN 250, ULF470: DN 300

Material: Foundation pipe: PE; Foundation slab: polymer concrete

Features: universal foundation system for various charging stations and charging pedestals; adaptation option for empty conduits; replacement or exchange of the charging station possible without removing the foundation

**Technical drawings**

[Zeichnung ULF380 (.PDF)](https://db.hauff-technik.de/files/1045/3/ULF380_1X110.PDF)

[Zeichnung ULF470 1x150 (.PDF)](https://db.hauff-technik.de/files/1045/3/ULF470_1X150.PDF)

[Zeichnung ULF300 (.PDF)](https://db.hauff-technik.de/files/1045/3/ULF300_1X110.PDF)

[Zeichnung ULF470 1x110 (.PDF)](https://db.hauff-technik.de/files/1045/3/ULF470_1X110.PDF)

Ctrl + click on the link to open in your browser

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de