**Sleeve**

for cable sealing at the end of the duct

Article Code: KES90 MA90-102/90-102 WE

GTIN: -

Brand: Hauff-Technik

For installation at the end of the Hateflex spiral duct 14090. In combination with the interchangeable insert WE 100-z/d, which is installed in the sleeve, cables can be sealed using rubber compression technology.

Material: Clamping straps: W4; Sleeve: EPDM

Tightness: gastight and watertight to 2.5 bar

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de