**Outer sealing element module 1**

for district heating multi-line building entry system basic variant 1

Article Code: MSH FW Basic M1

GTIN: -

Brand: Hauff-Technik

Extension module for district heating multi-line building entry system (wall-mounted) for buildings without structural seal.

Dimensions: Compatible with core drill/wall sleeve ID: 299 - 302 mm; Sealing width: 30 mm

Material: Die-cast aluminium with cathodic coating/EPDM

Application range: Waterproof concrete stress class 1 and 2

Features: visual installation reliability due to built-in inspection opening

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de