**Universal insulating plate module 3**

for district heating multi-line building entry system basic variant 1 and 2

Article Code: MSH FW Basic M3

GTIN: -

Brand: Hauff-Technik

For insertion in existing perimeter insulation, combined with MSH-FW outer sealing element module 1, module 5 or module 6.

Dimensions: OD: 440/299 mm; Insulation thickness: 50 mm

Material: Styrodur (EPS)

Features: predetermined breaking point ensures compatibility for use with various diameters

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de