**Outer sealing element module 5**

for district heating multi-line building entry system basic variant 1

Article Code: MSH FW Basic M5

GTIN: -

Brand: Hauff-Technik

Extension module for district heating multi-line building entry system without wall fitting for sealing in waterproof concrete core drills with integrated heat insulation. The sealing element can be pushed through the hole that has been drilled in the insulation and then positioned in the concrete.

Dimensions: Compatible with core drill/wall sleeve ID: 299 - 302 mm; Sealing width: 30 mm

Material: Die-cast aluminium with cathodic coating/EPDM

Application range: Waterproof concrete stress class 1 and 2

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de