**Standard press seal**

for building connections

Article Code: HSD100 EW 1x24-44+4x7-12 b40 A2/EPDM

GTIN: -

Brand: Hauff-Technik

Press seal for sealing cables/media pipes in core drills or wall sleeves. Closed design for sealing new lines to be installed. Tested according to FHRK test basis with FHRK quality seal.

Dimensions: Sealing width: 40 mm; For core drills/wall sleeves Ø: 100 mm; For 5 cables/pipes of which 4 x Ø 7-12 mm and 1 x Ø 24-44 mm

Material: Press plates, screws and nuts: rust-free stainless steel V2A (AISI 304L); Rubber: EPDM

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight; radon-proof

Features: Visual and physical installation control thanks to integrated inspection opening; integrated segmented ring technology for individual adjustment to cable diameters on site

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de