**Connection set for cable entry system with core drill holes/wall sleeve**

for retrofit installation

Article Code: KES150 MA KB SET

GTIN: -

Brand: Hauff-Technik

For connecting the Hateflex spiral duct 14150 to core drills or wall sleeves. The pipe socket is connected to the duct with a sleeve. Sealing is done with the two press seals (included in scope of delivery).

Dimensions: Pipe socket OD: 160 mm; Pipe socket length: 500 mm

Material: Sleeve/sealing rubber: EPDM; Clamping straps, press plates, screws, nuts: stainless steel V2A (AISI 304L); Pipe socket: PVC

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 2.5 bar

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de