**Split interchangeable insert with segment ring technology**

for cable sealing at the end of the duct

Article Code: WE160 SG

GTIN: -

Brand: Hauff-Technik

For installation within the KES150 MA WE sleeve to seal cables at the end of the Hateflex spiral duct 14150

Dimensions: OD: 160 mm; Sealing width: 60 mm; Maximum configuration: according to variant table

Material: EPDM

Tightness: gastight and watertight to 2.5 bar

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de